MAP OF HACKS FOR THE MOTOROLA Vxxx PHONE

Originally created and tested for TRIPLETS series phones V300/V400/V500/V600.

Extended to include features of V547/V551, V3RAZR, V635.

Not tested on V180/V220/V550/V620/V80/Axxx/Exxx/CDMA phones/etc, so use at your own risk on those phones.

Last Modified (GMT -0400) 7:49 AM Thursday, May 11, 2006

Latest Changes:
seem 0032, offset 96/AE (for V3i hacks)



seem 0032, offset 93/94 (for V3i hacks)



gain_table, offset 1BD (for V3i wired headset)



seem 0313/0314 (in other interesting seems)



seem 0032, offset 9A



gain_table volume step descriptions added



seem 0032, offset 8C, bit 2



kjava/j2me*.pat files



seem 0032, offset 69, bit 3



seem 0254 and 0278 added to other interesting seems (with details)



seem 004a, offset 1D1



seem 0032, offset 83, bit 4



added more gain_table hacks (microphone gains, master gain, volume control steps)



added more gain_table hacks (speakerphone keypad, voice name; bluetooth voice name/voice record)



added seem 004e for max video record size setting (V635)



added numerous gain_table hacks (wired headset gains, BT headset gains, voice name/voice record gains, system tone gains)



added some new seem 0032 hacks provided to me (mostly items that are set 'on' by default in almost all flexes)

What does this all mean?

See http://xlr8.us/hofo/ for a tutorial.

Disclaimer:

Use this information at your own risk! 

I cannot be held responsible if you damage your phone.

If you have questions, contact me via PM on http://www.howardforums.com/ - my handle is 'xlr8'. 

DO NOT E-MAIL ME ABOUT THIS. PM via Howard Forums only. 

By keeping this page open and reading the information below, you agree to these stipulations. 

========

Other Interesting Seems:

0002 - (Multiple Records) Shortcuts

0016 - Stores Hardware Version

0037 - (Multiple Records) Stores Quick Dial Numbers

0038 - (Multiple Records) Stores Received Numbers

0039 - (Multiple Records) Stores Dialed Numbers

005B - Key Mapping

0064 - SMS Service Center Number

0074 - Stores Phone Lock Code

0076 - Stores Phone Security Code

007D - (Multiple Records) SMS Messages (stored on phone)

00AE - (Multiple Records) Bluetooth Device History

0117 - Phone Model Number

0132 - Bluetooth Name

013A - Greeting Text

0171 - Other Information > Technology

017F - Flex Version

0254 - (Records 0001-0003) E-Mail Provider details (see also seem 0278): provider name begins at offset 09, with 00 between each character, offset 29 sets POP3/IMAP4 status (6E for port 110/pop3, 8F for port 143/impa4), offset 2B sets SMTP port number (25)

0259 - (Multiple Records) Phonebook Categories

026B - Lifetime Call Times

0278 - (Records 0001-0003) E-Mail Provider details (see also seem 0254): pop3/imap4 server name begins at offset 00 with _no_ 00 between each character, smtp server name begins at offset 42 with _no_ 00 between each character

02D2 - Firmware Version

02D3 - Flex Version

0313 - Carrier/Browser Key Assignment (use mma menu code)

0314 - Camera/Message Key Assignment (use mma menu code)

========

kjava/j2me*.pat files

Permission File for Each Installed Java Application (Games & Apps > menu > Permissions)

offset 06: determines selected option for Network Related > Data Network (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 07: determines available options for Network Related > Data Network (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 08: determines selected option for Network Related > Messaging (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 09: determines available options for Network Related > Messaging (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 0A: determines selected option for Network Related > App Auto-Start (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 0B: determines available options for Network Related > App Auto-Start (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 0C: determines selected option for Network Related > Connectivity Options (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 0D: determines available options for Network Related > Connectivity Options (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 0E: determines selected option for User Data Related > Multimedia Recording (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 0F: determines available options for User Data Related > Multimedia Recording (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 10: determines selected option for User Data Related > User Data Read Capability (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 11: determines available options for User Data Related > User Data Read Capability (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 12: determines selected option for User Data Related > User Data Write Capability (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 13: determines available options for User Data Related > User Data Write Capability (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

offset 14: determines selected option for User Data Related > App Data Sharing (00 for 'access denied', 01 for 'always ask', 02 for 'ask once per app', 04 for 'never ask')

offset 15: determines available options for User Data Related > App Data Sharing (00 for no access/item not displayed, 01 for 'always ask' option, 02 for 'ask once per app', 03 for 'never ask', 04 for full unprompted access)

========

plmn_text_table.bin

Alpha Tag Database

seem 0032, offset 4B, bit 6 must be set to "0"

in some cases, seem 0032, offset 02, bit 1 must be set to "0" also

first offset prior to text is the number of characters in the alpha tag, in hex

Example: "Cingular" would require "08" and "XLR8 Is Awesome" would require "0F"

Confusing?  Maybe so.  A little lesson for counting in hexadecimal.  Forget what you learned about counting to "10" in Kindergarten; let's count to "10" in hex...

00, 01, 02, 03, 04, 05, 06, 07, 08, 09, 0A, 0B, 0C, 0D, 0E, 0F, 10 (exciting, huh?  wanna count to "10" in binary?  00, 01, 10 EASY!)

second offset prior to text has something to do with the band the network uses (ie. 850/900/1800/1900)  I recommend not changing it.

It appears as though 01/02/03 denote 900/1800 and 04/08/0C denote 850/1900 and 05/07/09 denote all bands.

third offset prior to text is the first two digits of the "MNC" code, reversed

Example: For a network code of 123-456, you would see "54" in this offset

fourth offset prior to text is the last digit of the "MCC" code (digit #2 in the offset) and the last digit of the "MNC" code (digit #1 in the offset)

Example: For a network code of 123-456, you would see "63" in this offset

fifth offset prior to text is the first two digits of the MCC code, reversed

Example: For a network code of 123-456, you would see "21" in this offset

========

gain_table.bin

**all offsets are HEX**

**no bit manipulation here, just change the actual value of the offset**

SPEAKER GAINS

offset 0D earpiece call gain (original setting: 01, recommended setting: 05) (master control at offset 10: 08)

offset 19 earpiece keypad gain (original setting: 01, recommended setting: 01) (master control at offset 1E: 08)

offset 25 earpiece system tone gain (original setting: 01, recommended setting: 08) (master control at offset 2A: 08)

offset 31 external speaker speakerphone gain (original setting: 01, recommended setting: 03) (master control at offset 34: 08)

offset 3D external speaker keypad gain when on speakerphone call (original setting: 01, recommended setting: 01) (master control at offset 40: 08)

offset 49 external speaker mp3/midi/video gain (original setting: 01, recommended setting: 03) (master control at offset 4C: 08)

offset 4E external speaker system tone gain (original setting: 08, recommended setting: 01)

offset 61 wired headset call gain (original setting: 02, recommended setting: 05) (master control at offset 64: 08)

offset 6D wired headset inner keypad gain (original setting: 01, recommended setting: 01) (master control at offset 72: 08)

offset DC bluetooth headset call gain (original setting: 08, recommended setting: 0F)

offset EA bluetooth headset inner keypad gain (original setting: 08, recommended setting: 08)

offset F6 external speaker system tone gain when bluetooth headset connected (original setting: 08, recommended setting: 01)

offset 139 earpiece voice name/voice record playback gain (original setting: 01, recommended setting: 05) (master control at offset 13C: 08)

offset 145 wired headset mp3/midi/video gain (original setting: 02, recommended setting: 04) (master control at offset 148: 08)

offset 15D external speaker voice dial gain when on speakerphone call (original setting: 01, recommended setting: 03) (master control at offset 160: 08)

offset 178 bluetooth voice name/voice record playback gain (original setting: 08, recommended setting: 0F)

offset 1BD V3i wired headset mp3/midi/video gain (original setting: 01, recommended setting: 04) (master control at offset 1C0: 08)

MICROPHONE GAINS

offset 1E1 handset microphone gain (original setting: 0E, recommended setting: 0F) (V3/RAZR original setting: 19, recommended setting: 15)

offset 1F9 wired headset microphone gain (original setting: 1F, recommended setting: 1F) (V3/RAZR original setting: 00 ???)

offset 21D speakerphone microphone gain (original setting: 1F, recommended setting: 1F)

offset 238 bluetooth headset microphone gain (original setting: 08, recommended setting: 1B)

MASTER GAIN

offset 3A6 master gain control for speakers and microphones (original setting: 08, recommended setting: 08)

MASTER VOLUME CONTROL STEPS (controls master gain, but only at the specific volume level on the phone)

offset 3A9 master gain volume step 0 (original setting: 00, recommended setting: 00)

offset 3AB master gain volume step 1 (original setting: 01, recommended setting: 01)

offset 3AD master gain volume step 2 (original setting: 02, recommended setting: 02)

offset 3AF master gain volume step 3 (original setting: 03, recommended setting: 03)

offset 3B1 master gain volume step 4 (original setting: 04, recommended setting: 04)

offset 3B3 master gain volume step 5 (original setting: 05, recommended setting: 05)

offset 3B5 master gain volume step 6 (original setting: 06, recommended setting: 07)

offset 3B7 master gain volume step 7 (original setting: 07, recommended setting: 09)

settings from 00 and up; remember to count in hex... you don't go directly from 09 to 10... it goes 09 0A 0B 0C 0D 0E 0F 10

earpiece call gain sounds coming out of the earpiece when on a call

earpiece inner keypad gain affects sounds coming out of the earpiece when NOT on a call (touchtones, button press beeps)

earpiece system tone gain affects system tones coming out of the earpiece when on or attempting a call (call drop tone, voice dial failed tone, call failed tone, headset disconnect tone)

external speaker speakerphone gain affects sounds coming out of the external speaker when on a call with speakerphone activated

external speaker keypad gain when on speakerphone call affects keypress sounds and system tones coming out of the external speaker when on a call with speakerphone activated

external speaker mp3/midi/video gain affects multimedia, mp3, and midi sounds coming out of the external speaker (includes midi/mp3 tones, video playback)

external speaker system tone gain effects system tones coming out of the external speaker (reminder tone, style/volume change tone, Continental/Siren/Attention/Classic ringtones, low batt tone, service tone, autoredial ring, roaming ringtone)

wired headset call gain affects sounds coming out of the wired headset when on a call

wired headset inner keypad gain affects sounds coming out of the wired headset when NOT on a call (touchtones, button press beeps)

bluetooth headset call gain affects sounds coming out of the bluetooth headset when on a call

bluetooth headset inner keypad gain affects sounds coming out of the bluetooth headset when NOT on a call (touchtones, button press beeps)

external speaker system tone gain when bluetooth headset connected affects ALL SOUNDS coming out of the phone when a bluetooth headset is connected (because only system tones can come out of a motorola phone when a bluetooth headset is connected)

earpiece voice name/voice record playback gain affects sounds coming out of the earpiece during playback of voice records, scrolling through phonebook entries with a voice name, and name confirmation during voice dial

wired headset mp3/midi/video gain affects multimedia, mp3, and midi sounds coming out of a wired headset when connected (includes midi/mp3 tones, video playback)

external speaker voice dial gain when on speakerphone call affects sounds coming out of the external speaker when browsing phonebook entries with voice names

bluetooth voice name/voice record playback gain affects sounds coming out of the bluetooth headset during playback of voice records, scrolling through phonebook entries with a voice name, and name confirmation during voice dial

handset microphone gain affects the sensitivity of the microphone when on a call

wired headset microphone gain affects the sensitivity of the microphone when on a call with a wired headset connected

speakerphone microphone gain affects the sensitivity of the microphone when on a call with speakerphone activated

bluetooth headset microphone gain affects the sensitivity of the microphone when on a call with a bluetooth headset connected

master gain control affects all sounds coming out of all speakers and the sensitivity of all phone microphones

volume control steps affect the gain of individual volume control levels of the phone

========

SEEM 00a2_0001

**all offsets are HEX**

offset 00 -
bit 5: disable AMR Half Rate (1 on, 0 off) (bit 6 must be off)



bit 6: enable AMR Half Rate (1 on, 0 off) (bit 5 must be off)

offset 01 -
bit 5: disable AMR Full Rate (1 on, 0 off) (bit 6 must be off)



bit 6: enable AMR Full Rate (1 on, 0 off) (bit 5 must be off)

How to tell what audio codec your phone is using:

While in a call, enter field test mode and in the Serving CS/TB screen, look on the bottom line beside "coder."

The first part of that string of letters is the part you're looking for.

AFS = AMR Full Rate

AH0 = AMR Half Rate

AH1 = AMR Half Rate

EFR = Enhanced Full Rate

FR = Full Rate

========

SEEM 010a_0001

**all offsets are HEX**

offset 00 -
bit 0: GPRS auto-attach at power-on (1 on, 0 off) (if bit 1 is on, auto-attach will be off)



bit 1: GPRS detach after GPRS data session (bit 0 must be on to activate)

========

SEEM 01a8_0001 controls Date/'GPRS' displayed in second line of home screen under carrier name

========

SEEM 004a_0001

**all offsets are HEX**

**no bit manipulation here, just change the actual value in the offset**

offset 22 (01 for custom startup sound stored in /a/mobile/audio/Start~up.mp3, 00 for no custom startup sound), may need to adjust 0032_0001, offset 24, bit 3

offset 23 (01 for custom startup in stored seems 0206/0208, 00 for no custom startup)

offset 24 (01 for custom shutdown sound stored in /a/mobile/audio/Power~down.mp3, 00 for no custom shutdown sound)

offset 27 (00 for custom outer image from path saved in seems 0061/0062, 01 for custom outer text stored in seems 0061/0062, 02 for Motorola icon)

offset 80 (01 for number display with no dashes, 00 for number display with dashes- 1-404-555-1212)

offset 148 (01 for MTWTFSS week format in calendar, 00 for SMTWTFS week format in calendar)

offset 1BE (00 for no deletion of inbox, outbox, drafts messages on sim swap)

offset 1C0 (01 for blue hellomoto splash screen, 00 for original hellomoto splash screen)

offset 1D1 (01 for .3gp video record, 03 for .mp4 video record)

offset 1D3 (01 for Multimedia > Video Camera, 00 for no Video Camera) (see also seem 0032, offset 60, bit 6)

========

SEEM 004e_0001

**all offsets are HEX**

**no bit manipulation here, just change the actual value in the offset**

offset 412 -
controls video record file size when phone setting is "maximum"



set to 01 for a max size of ~1 Megabyte (0100hex = 1024 kilobytes = 1 mb)



set to 14 for a max size of ~5 Megabytes (1400hex = 5120 kilobytes = 5 mb)



set to 28 for a max size of ~10 Megabytes (2800hex = 10240 kilobytes = 10 mb)



etc.

========

SEEM 0025_0001

**all offsets are HEX**

offset 00 - 
bit 0, bit 3: 900/1800 and 1900 (set each of these bits to 1)



bit 0, bit 1, bit 3: 850/1900 and 900/1800 (set each of these bits to 1)



bit 0, bit 2, bit 3: 850/1900 and 900 (set each of these bits to 1)



bit 2, bit 3: 850/1900 and 1800 (set each of these bits to 1)

========

SEEM 0126_0001

**all offsets are HEX**

offset 00 -
bit 7: Display My Phone Number at Power On (0 fix enabled, 1 fix not enabled) (offset 04 MUST Be Set - Fix for S/W >38R)

offset 02 -
bit 1: House Icon and "Home" Displayed when in "Homezone" (provider specific, O2 Germany) (1 on, 0 off)



bit 5: Settings > Phone Status > My Tel. Numbers - store number after restart fixed for S/W .38R and above (1 fix enabled, 0 fix not enabled)

offset 03 -
bit 5: Items Displayed in Recent Calls > Dialed Calls (1 to display only most recent call to same number, 0 to display all calls to the same number)



bit 6: Items Displayed in Recent Calls > Received Calls (1 to display only most recent call from same number, 0 to display all calls from the same number)

offset 04 - 
bit 5: Display My Phone Number at Power On (1 fix enabled, 0 fix not enabled) (offset 00 MUST Be Set - Fix for S/W >38R)

========

SEEM 0061_0001 - determines external LCD display text when flip is open aka "Cingular"

SEEM 0062_0001 - determines external LCD display text when flip is open aka "Cingular"

========

mma_ucp & mma_dcp

controls menus

menu codes:

"FEM" for Engineering Menu

"AIM" for AIM

"IM" for IM

"MobileQQ" for MobileQQ

"Video" for Videos (no 's' on the menu code)

"Bluetooth" for Bluetooth

"CDAG" for Quick Menu

"Chat" for Chat

"VideoCamera" for Video Camera

"AirplaneMod" for Airplane Mode (does not work on most phones, confirmed on A630 only)

========

SEEM 0032_0001

bits: 00000000 <-- binary

      76543210 <-- bit #

**all offsets are HEX**

offset 00 -
bit 0: Settings > Initial Setup > Time and Date > Autoupdate Menu (1 on, 0 off)



bit 1: Settings > Initial Setup > Time and Date > date setting option (1 on, 0 off)



bit 2: Settings > Initial Setup > Auto Redial (1 on, 0 off)



bit 6: Settings > Phone Status > Other Information (1 on, 0 off)



bit 7: Settings > Phone Status > Other Information > S/W Version, DSP S/W Version, Language List (1 on, 0 off)

offset 01 -
bit 0: Settings > Phone Status > Other Information > PRL Version (1 on, 0 off)



bit 1: Settings > Phone Status > Other Information > Data Ready (1 on, 0 off)



bit 2: Settings > Phone Status > Other Information > TrueSync Ready (1 on, 0 off)



bit 3: Settings > Phone Status > Other Information > Browser Ready (1 on, 0 off)



bit 5: SIM capable device (1 on, 0 off)

offset 02 -
bit 0: Settings > In-Call Setup > Answer Options > Open To Answer (1 on, 0 off)



bit 1: BLOCKS THESE FEATURES: Call barring, Call transfer, Info Services, do not read VM number from SIM, Voicemail ^@ text messages, Multi-Line Support, My Network List, Manual Network Search (1 on, 0 off - set to 0 to UNBLOCK these features) 



some of these features may be SIM dependant anyway, so activating it on your phone may not actually allow you to use it



bit 4: ^@ and _@ VM Indicator SMS Msgs (1 off, 0 on) (**DOES NOT WORK RELIABLY**)



bit 7: Message > Info Services (1 on, 0 off)

offset 03 -
bit 1: Message > Quick Notes (1 on, 0 off)



bit 2: Message > Drafts (1 on, 0 off)



bit 3: Message > Outbox (1 on, 0 off)



bit 5: Message > Inbox (1 on, 0 off)



bit 6: Settings > Ring Styles > Details > Ans Mach option (1 on, 0 off)



bit 7: Alarms Available (1 on, 0 off)

offset 04 - 
bit 1: Call Restriction Support (1 on, 0 off)

offset 05 - 
bit 3: Silent alert (ringtones) (1 on, 0 off)

offset 06 - 
bit 1: Siren alert (1 on, 0 off)

offset 08 -
bit 2: Office Tools > Voice Records (1 on, 0 off)



bit 3: Allow Voicenote for Datebook (1 on, 0 off)



bit 4: Allow Voicenote for Ring Alerts (1 on, 0 off)



bit 5: Recent Calls > Call Cost (1 on, 0 off)



bit 7: Phonebook > Edit > Voice Name (1 on, 0 off)

offset 09 - 
bit 0: Voice Dialing Support (1 on, 0 off)



bit 1: Settings > Security > Talk Secure (1 on, 0 off)



bit 3: Settings > Security > Lock Application > Recent Calls (1 on, 0 off)



bit 4: Settings > Security > Lock Application > Phonebook (1 on, 0 off)



bit 5: Settings > Security > Lock Application > Datebook (1 on, 0 off)



bit 6: Settings > Security > Lock Application > Radio (1 on, 0 off)



bit 7: Settings > Security > Lock Application > Messaging (1 on, 0 off)

offset 0A - 
bit 0: Settings > Security > Lock Application > Shortcuts (1 on, 0 off)



bit 1: Settings > Security > Lock Application > SIM Apps (1 on, 0 off)



bit 2: Settings > Security > Lock Application > Browser (1 on, 0 off)



bit 3: Phonebook > Edit > Insert P (Pause) (1 on, 0 off)



bit 4: Phonebook > Edit > Insert W (Wait) (1 on, 0 off)



bit 5: Phonebook > Edit > Insert N (Number) (1 on, 0 off)



bit 6: iTAP Support (1 on, 0 off)



bit 7: Settings > Initial Setup > Backlight > Continuous option (1 on, 0 off)

offset 0B -
bit 0: Settings > Phone Status > Other Information > ESN (1 on, 0 off)



bit 2: GSM Phone Available (1 on, 0 off)



bit 3: Automatic Lanaguage Support (1 on, 0 off)

offset 0C -
bit 0: Multiple Language Support (1 on, 0 off)



bit 1: Menu: Smart Key (1 on, 0 off)



bit 6: Menu: Services (1 on, 0 off)

offset 0D -
bit 4: Recent Calls > Detail (1 on, 0 off)



bit 7: Settings > Connection > Bluetooth (1 on, 0 off) (menu item, may require update to mma files)

offset 0E -
bit 0: Retrieve IMEI by pressing *#06# (1 on, 0 off)



bit 1 - Subsidy Lock Available (1 on, 0 off)



bit 4 - GSM 900MHz Capable (1 on, 0 off)



bit 5 - GSM 1800MHz Capable (1 on, 0 off)



bit 6 - GSM 1900MHz Capable (1 on, 0 off)

offset 0F - 
bit 0: Browser Additional Charge Prompt (1 on, 0 off)

offset 13 - 
bit 0: Multimedia > Radio (1 on, 0 off)



bit 6: "City" Displayed when in certain areas (provider specific, O2 Germany) (1 on, 0 off)

offset 14 - 
bit 0: Settings > In-Call Setup > My Caller ID > All Calls (1 on, 0 off)



bit 1: Office Tools > SIM Applications (1 on, 0 off)



bit 2, 3: Office Tools > Dialing Services > Quick Dial (1 on, 0 off) (bit 2 can cause Settings > Personalize menu to hang) (menu item, may require update to mma files)



bit 4: Settings > Network > Current Network (1 on, 0 off)



bit 5: Settings > Network > New Network (1 on, 0 off)



bit 6: Settings > Network > Network Setup (1 on, 0 off)



bit 7: Settings > Network > Search Type (1 on, 0 off)

offset 15 - 
bit 2: Settings > Network > Available Networks (1 on, 0 off)



bit 3: Settings > Network > My Network List (1 on, 0 off)



bit 4: Settings > Network > Service Tone (1 on, 0 off)



bit 5: Settings > Network > Call Drop Tone (1 on, 0 off)



bit 7: Allow CALL BAR Password Change (1 on, 0 off)

offset 16 - 
bit 6: Settings > Ring Styles > Details > Roam Calls option, special ring tone for calls received while roaming (1 on, 0 off)



bit 7: Allow Numeric Text Entry (1 on, 0 off)

Offset 17 -
bit 2: Allow TAP Text Entry (1 on, 0 off)



bit 6: Settings > Phone Status > Other Information > Technology (1 on, 0 off)



bit 7: GPRS Capable (1 on, 0 off)

offset 18 - 
bit 0: Browser Display CSD Dialogue (Warn User of CSD Call) (1 on, 0 off)



bit 4: WebAccess > Browser > Menu > Set Homepage (1 on, 0 off)



bit 5: WebAccess > Browser Setup (1 on, 0 off)



bit 6: Webaccess > Web Sessions > Edit > UserID (1 on, 0 off)



bit 7: Webaccess > Web Sessions > Edit > Password (1 on, 0 off)

offset 19 -
bit 0: Webaccess > Web Sessions > Edit > CSD (1 on, 0 off)



bit 1: Webaccess > Web Sessions > Edit > Timeout (1 on, 0 off)



bit 2: Webaccess > Web Sessions > Edit > Line Type (1 on, 0 off)



bit 3: WebAccess > Browser Setup > Confirmation option (1 on, 0 off)



bit 4: WebAccess > Browser Setup > Cache Startup (1 on, 0 off)

offset 1A -
Bit 0: CSD Capable (Circuit Switched Dialing) (1 on, 0 off)



Bit 2: Browser: CSD Errors are Transparent (1 on, 0 off)



Bit 6: Browser: Homepage Available (1 on, 0 off)

offset 1B -
bit 0: Browser: OTA Provisioning Available (1 on, 0 off)



bit 3: Media Center > Incoming Call (1 on, 0 off)



bit 5: SIMTK Sustain Call (1 on, 0 off)



bit 6: Settings > Initial Setup > Auto PIN Dial (1 on, 0 off)



bit 7: Settings > Initial Setup > 1-Touch Dial (1 on, 0 off)

offset 1C -
bit 0: Settings > Initial Setup > Preferred Card (1 on, 0 off)



bit 3: Browser: Standard Provisioning (1 on, 0 off)



bit 6: Settings > Connection > IrDA available (1 on, 0 off)



bit 7: Settings > In-Call Setup > My Caller ID (1 on, 0 off)

offset 1D -
bit 0: External LCD Backlight (1 always on when flip closed, 0 on briefly when flip closed)



bit 3: Moto Startup Animation (1 on, 0 off)



bit 4: Security/PIN Code Support (1 on, 0 off)



bit 5: In-Call: Speed Dial (1 on, 0 off)



bit 6: Settings > Initial Setup > Battery Save (1 on, 0 off)

offset 1E - 
bit 0: Keypad: Voicerecord Key Available (Side Key) (1 on, 0 off)



bit 2: Bluetooth Headset Support (1 on, 0 off)



bit 3: Settings > Initial Setup > Animation (1 on, 0 off)



bit 6: Message > Menu > Message Setup > Expire After (1 on, 0 off)



bit 7: Settings > In-Call Setup > Talk and Fax > All Calls (1 on, 0 off)

offset 1F -
bit 0: Settings > In-Call Setup > Call Waiting (1 on, 0 off)



bit 1: CSD (Circuit Switched Dialing) (1 on, 0 off)



bit 2: General Cell Broadcast (1 on, 0 off)



bit 3: Message > Info Services Setup (1 on, 0 off)



bit 4: Settings > Phone Status > Active Line (Multi-Line Support) (1 on, 0 off)



bit 5: Settings > Security > Call Barring (1 on, 0 off)



bit 6: Data Calls (1 on, 0 off)



bit 7: Fax Calls (1 on, 0 off)

offset 20 -
bit 0: Messages > Voicemail (1 on, 0 off)



bit 1: Settings > In-Call Setup > Talk and Fax (1 on, 0 off)



bit 6: Recent Calls > Call Cost configuration (1 on, 0 off)

offset 22 -
bit 5: Settings > Call Divert/Forward > Voice Calls (1 on, 0 off)



bit 6: Settings > Call Divert/Forward > Fax (1 on, 0 off)



bit 7: Settings > Call Divert/Forward > Data Calls (1 on, 0 off)

offset 23 - 
bit 1: In-Call: Call Hold (1 on, 0 off)



bit 2: Settings > Call Forward (1 on, 0 off)



bit 5: Settings > In Call Setup > Call Guard option (1 on, 0 off)

offset 24 -
bit 2: Press & Hold 1 to Autodial Voice Mail Number (1 on, 0 off)



bit 3: Custom Startup Sound (004a_0001, offset 22 must be set to 01) (1 on, 0 off)

offset 26 - 
bit 2: v.42BIS Compression Available for CSD (1 on, 0 off)



bit 5: GSM Dual-Band Phone (1 on, 0 off)

offset 27 - 
bit 4 - MT CSD Support (1 on, 0 off)

offset 28 - 
bit 5: Phonebook: Edit Name (1 on, 0 off)



bit 6: Phonebook: Edit Number (1 on, 0 off)

offset 29 -
bit 1: Settings > Security > Lock Keypad (1 on, 0 off)



bit 2: Menu + # > My Phonenumber (1 on, 0 off)

offset 2B - 
bit 0: Test Mode On (1 on, 0 off) (allows "menu 0 0 * * T E S T M O D E *" to enable field test mode)



bit 1: Test Mode Off (1 on, 0 off) (allows "menu 0 0 * * T E S T O F F *" to disable field test mode)



bit 3: Settings > Initial Setup > Language (1 on, 0 off)



bit 4: Settings > Initial Setup > Contrast (1 on, 0 off)



bit 7: Allow Lock-Code Change (1 on, 0 off)

offset 2C -
bit 4: Roaming Menu (1 on, 0 off)

offset 2F -
bit 1: WebAccess > Web Sessions Menu (1 on, 0 off) (menu item, may require update to mma files)



bit 2: Webaccess > Web Sessions > Edit > IP1 (1 on, 0 off)



bit 3: Webaccess > Web Sessions > Edit > IP2 (1 on, 0 off)



bit 4: Webaccess > Web Sessions > Edit > CSD1 (1 on, 0 off)



bit 5: Webaccess > Web Sessions > Edit > CSD2 (1 on, 0 off)



bit 6: AUTO APN - Queries GGSN for Default APN if Blank in Websession (1 on, 0 off)



bit 7: Time to hold power button down to power on phone (1 instant, 0 press and hold)

offset 30 -
bit 1: Motorola Greeting Tone Available (1 on, 0 off)



bit 5: Office Tools > Dialing Services > Quick Dial (allow edit) (1 on, 0 off)



bit 6: Settings > Personalize > Home Screen > Banner (1 on, 0 off) (text in 0063_0001)



bit 7: Settings > Personalize > Greeting (1 on, 0 off) (text in 013a_0001)

offset 31 - 
bit 0: Moto Shutdown Animation (1 on, 0 off)



bit 4: Settings > Security > Lock Application > Voice Notes (1 on, 0 off)



bit 5: Settings > Security > Lock Application > Settings (1 on, 0 off)



bit 7: Settings > Security > Lock Application > Roaming (1 on, 0 off)

offset 32 -
bit 0: Settings > Security > Lock Application > Service Dial (1 on, 0 off)



bit 1: Settings > Security > Lock Application > Quick Dial (1 on, 0 off)



bit 2: Settings > Security > Lock Application > Messaging (1 on, 0 off)

offset 33 -
bit 6: Settings > Initial Setup > Backlight > Color (1 on, 0 off)

offset 34 -
bit 3: Display Roam Triangle Icon (1 on, 0 off)



bit 5: Office Tools > Datebook (1 on, 0 off)



bit 6: Settings > Phone Status > Other Information > PRI Checksum (1 on, 0 off)

offset 36 -
bit 2: Settings > Phone Status > My Tel. Numbers (1 on, 0 off)



bit 4: Opcode Menu (Menu->048263*) Available (1 on, 0 off)

offset 37 -
bit 1: *#9999# from home screen shows "Other Information" menu (1 on, 0 off)



bit 2: Settings > Initial Setup > Status Light (1 on, 0 off)



bit 3: Office Tools > Calculator (1 on, 0 off)

offset 38 - 
bit 1: Continental alert (1 on, 0 off)



bit 2: Classic alert (1 on, 0 off)



bit 3: Attention alert (1 on, 0 off)

offset 3B -
bit 2: Vibe Dot alert (1 on, 0 off)



bit 3: Vibe Dash alert (1 on, 0 off)



bit 4: Vibe Dot Dot alert (1 on, 0 off)



bit 5: Vibe Dot Dash alert (1 on, 0 off)



bit 6: Vibe Pulse alert (1 on, 0 off)

offset 3C -
bit 7: SMS Allow Multiple Destinations (1 on, 0 off)

offset 3D -
bit 0: E-Mail via SMS (1 on, 0 off)



bit 1: SMS delivery reports (1 on, 0 off)



bit 3: Message Character Counts (0 for up, 1 for down) (only works on phones with TRIPLETS firmware)



bit 5: EMS via SMS (Enhanced Messaging Service) (1 on, 0 off)



bit 7: Message > Inbox Setup > Email Gateway (1 on, 0 off) see 56/4 also

offset 3E -
bit 4: for purposes of linking name in phonebook with caller ID number, xxx-xxxx = xxx-xxx-xxxx = 1-xxx-xxx-xxxx = +1-xxx-xxx-xxxx (0 on, 1 off)



bit 5: Office Tools > Quick Menu (1 on, 0 off) (menu item, may require update to mma files)



bit 7: Recent Calls > Call Times > Reset (1 on, 0 off)

offset 3F -
bit 4: SMS Unicode (1 on, 0 off)



bit 6: Settings > Security > Restrict Calls (1 on, 0 off)

offset 40 -
bit 1: Display 'GPRS Attached' icon (1 on, 0 off)



bit 3: Display: Show Credit Remaining on Idle (1 on, 0 off)



bit 4: toggles forced display of provider information from SIM (ie "www.fido.ca") in second line (1 on, 0 off)



bit 6: SMS storage (0 for phone, 1 for SIM)

offset 41 -
bit 0: Datebook (C550) (1 on, 0 off)



bit 2: Display Foreign Carrier Name from SIM under Provider Name (1 show date always, 0 show foreign carrier name)



bit 5: Display: GPRS Icon Indicates Current Status (1 on, 0 off)



bit 6: Swap Delete Confirmation Key Position (1 on, 0 off)



bit 7: Allow CLI Send (Calling Line Identifier) (1 on, 0 off)

offset 43 -
bit 0: Settings > Java Settings > Java App Loader (1 on, 0 off)



bit 1: Settings > Java Settings > Delete All Apps (1 on, 0 off)



bit 2: Browser: Browser Msgs (1 on, 0 off)



bit 4: GSM Multi-Band Region Support for Automatic Scan (See Ofs 43 Bit 5) (1 on, 0 off)



bit 5: Settings > Network > Network Setup > Band > Automatic (1 on, 0 off)



bit 6: Settings > Personalize > Screensaver (1 on, 0 off)



bit 7: Multimedia > Pictures (Picture Viewer) (1 on, 0 off)

offset 44 -
bit 0: Settings > Personalize > Wallpaper (1 on, 0 off)



bit 1: Settings > Security > Lock Application > Pictures (1 on, 0 off)



bit 2: SMS: MO Concatenation (1 on, 0 off)



bits 4, 5, 6, 7: Office Tools > Engineering (1 on, 0 off) (menu item, may require update to mma files)

offset 45 -
bit 0: Keypad: Combined Power and End Key (1 on, 0 off)



bit 7: Settings > Phone Status > Other Information > MP3 Ready (1 on, 0 off)

offset 46 -
bit 0: Custom Shutdown Animation in seems 0207/0209 (1 on, 0 off)



bit 3: Messages > Menu > Message Setup > Message/Service Center Number (1 on, 0 off)



bit 4: Messages > Menu > Voicemail Setup (1 on, 0 off)



bit 6: Office Tools > Chat (1 on, 0 off) (menu item, may require update to mma files)



bit 7: Datebook Alarms (1 on, 0 off)

offset 47 -
bit 0: Settings > Security > Lock Application > Calculator (1 on, 0 off)



bit 1: Settings > Security > Lock Application > Games and Apps (1 on, 0 off)



bit 3: Settings > Initial Setup > TTY (1 on, 0 off)



bit 7: SMS CAPS lock (1 ABC, 0 Abc)

offset 48 -
bit 1: Display My Phone Number at Power On (1 on, 0 off) (see SEEM 0126_001 for S/W .38R and above)



bit 3: Browser > Menu > Bookmarks (1 on, 0 off)



bit 4: Settings > Call Divert/Forward > Voice Calls > Conditional (1 on, 0 off)



bit 5: Settings > Call Divert/Forward > Voice Calls > Busy (1 on, 0 off)



bit 6: Settings > Call Divert/Forward > Voice Calls > No Answer (1 on, 0 off)



bit 7: Settings > Call Divert/Forward > Voice Calls > Not Reachable (1 on, 0 off)

offset 49 -
bit 2: Right Soft Key Edit Available (1 on, 0 off)



bit 3: SMS forwarding header (prepends to subject line when forwarding a message) (1 add header, 0 no header)



bit 5: Web Access > Browser custom animated splash screen stored in /a/mib_op_greet (1 on, 0 off) (if set to 0, offset 1D, bit 3 will control whether or not a default motorola animation will display)



bit 7: Keypad: 4-Way Navigation Key (1 on, 0 off)

offset 4A -
bit 0: Settings > Personalize > Banner Graphic (1 on, 0 off)



bit 1: Message > E-Mail Msgs (1 on, 0 off)



bit 4: Settings > Security > Lock Application > Ring Styles (1 on, 0 off)



bit 5: Display: SMS Show Sender ID First on Preview (1 on, 0 off)



bit 6: toggles display of "Emergency Only" when a home or ok-to-roam network cannot be found, but another network is available (1 on, 0 off)



bit 7: toggles display of "No Service" when network cannot be found (1 on, 0 off) (this fixes the "No Service" display overwriting the time on the exterior LCD)

offset 4B -
bit 0: Recent Calls > Data Times (1 on, 0 off) (offset 4B, bit 3 must be set to 1)



bit 1: Recent Calls > Data Volumes (1 on, 0 off) (offset 4B, bit 3 must be set to 1)



bit 2: Byte Usage Summary at End of GPRS Session (xxx bytes transferred) (1 on, 0 off)



bit 3: Activate Recent Calls > Data counters (1 activated, 0 deactivated) (must activate specific menu items at offset 4B, bits 0 and 1)



bit 4: Recent Calls > Data Times/Volumes > Recent/All Data Sessions > Internal Data Session (1 on, 0 off) (offset 4B, bit 3 must be set to 1; offset 4B, bit 0, 1, or both must also be set to 1)



bit 5: Settings > Security > Lock Application > Chat (1 on, 0 off)



bit 6: Alpha Tag Display (1 from SIM, 0 from phone)



bit 7: Settings > Security > Lock Application > Call Divert/Forward (1 on, 0 off)

offset 4C -
bit 0: Settings > Security > Lock Application > Phone Status (1 on, 0 off)



bit 1: Settings > Security > Lock Application > Connections (1 on, 0 off)



bit 2: Settings > Security > Lock Application > In-Call Setup (1 on, 0 off)



bit 3: Settings > Security > Lock Application > Personalise (1 on, 0 off)



bit 4: Settings > Security > Lock Application > Initial Setup (1 on, 0 off)



bit 5: Settings > Security > Lock Application > Car Settings (1 on, 0 off)



bit 6: Settings > Security > Lock Application > Headset (1 on, 0 off)



bit 7: Settings > Security > Lock Application > Audio Player (1 on, 0 off)

offset 4D -
bit 0: Settings > Security > Lock Application > Video Player (1 on, 0 off)



bit 1: Settings > Security > Lock Application > Security (1 on, 0 off)



bit 2: Settings > Security > Lock Application > Network (1 on, 0 off)



bit 4: Browser: Numbered Options Support (Press 3 for Item 3 etc.) (1 on, 0 off)



bit 5: Browser: Send SI SL In Accept Headers (Required for WAP 2.0) (1 on, 0 off)



bit 6: Browser: Accept Headers Control Available (Set to OFF for T-Mobile US) (1 on, 0 off)

offset 4F -
bit 2: CHAP over GPRS Support (1 on, 0 off)



bit 6: Browser: Allow Back Button on Blank WML Page (1 on, 0 off)



bit 7: Browser: Disallow Browser Content Forwarding (1 on, 0 off)

offset 50 -
bit 0: 850 MHz Capable (1 on, 0 off)



bit 1: Webaccess (1 on, 0 off)



bit 7: Settings > In Call Setup > MSG Alert option (1 on, 0 off)

offset 51 -
bit 2: Messaging > Menu > Reorder (1 on, 0 off)



bit 3: Messaging > Create Message (1 on, 0 off)



bit 5: Multimedia > Motomixer (1 on, 0 off) (menu item, may require update to mma files)



bit 6: Voice Commands (use Menu+voice key) (0 on, 1 off)



bit 7: Multimedia > Themes (1 on, 0 off) (menu item, may require update to mma files)

offset 52 - 
bit 0: Multimedia > Themes > Setup > Delete (1 on, 0 off)



bit 6: Office Tools > AIM (1 on, 0 off) (menu item, may require update to mma files)



bit 7: Settings > Security > Lock Application > AIM (1 on, 0 off)

offset 53 -
bit 1: MT EMS Message Allow MIDI (1 on, 0 off)



bit 3: Show Personalize Phone Dialog on Reset or New SIM (1 on, 0 off)



bit 4: Settings > Security > Lock Application > Webaccess (1 on, 0 off)



bit 6: Settings > Personalize > Color Styles (allows for custom color style, upload spcolor.sch to /a/mobile/system/) (1 on, 0 off)



bit 7: Settings > Security > Lock Application > Skins/Color Style (1 on, 0 off)

offset 54 -
bit 0: Settings > Personalise > Skins/Color Style (1 on, 0 off)



bit 1: Default Skin/Color Style Available (1 on, 0 off)



bit 2: Office Tools > Mobile QQ (1 on, 0 off) (menu item, may require update to mma files)



bit 3: Settings > Security > Lock Application > Mobile QQ (1 on, 0 off)



bit 4: Webaccess > Bookmarks: Shorcuts: 50 URL's Supported (1 on, 0 off)



bit 5: Delete Confirmation (1 on, 0 off)



bit 6: function of right soft key when reading SMS message (0 delete, 1 reply)



bit 7: BLOCK ADVANCED MENUS: Settings > Network (1 on, 0 off - set to 0 to UNBLOCK advanced Network Menus)

offset 55 - 
bit 2: Time Autoupdate (1 on, 0 off) <-- this will actually activate the feature, the menu item is in offset 00



bit 3: HTTP OTA Client (1 on, 0 off)



bit 4: Settings > Initial Setup > Time and Date (Allow Change) (1 on, 0 off)



bit 5: GSM Multi-Band Phone (1 on, 0 off)

offset 56 - 
bit 1: Browser: Disable Store as Wallpaper for Graphics (1 on, 0 off)



bit 2: Browser: Browser > Menu > Home (1 on, 0 off)



bit 4: Messages > Inbox Setup > E-Mail Gateway (1 on, 0 off) see 3D/7 also



bit 6: SIM Language Support (1 on, 0 off)

offset 57 -
bit 2: Reduced Ringback (Redial) (1 on, 0 off)

offset 58 -
bit 1: Office Tools (1 on, 0 off)



bit 4: Office Tools > Shortcuts, list web shortcuts also (1 don't list, 0 list them)



bit 5: URL Shortcut Edit (1 on, 0 off)



bit 6: Phonebook > Menu > Copy > All to SIM/Phone Memory (1 on, 0 off)

offset 59 -
bit 4: Office Tools > Alarm Clock (1 on, 0 off)



bit 5: Settings > Security > Lock Application > Alarm Clock (1 on, 0 off)



bit 7: ITAP: Smart Punctuation (1 on, 0 off)

offset 5A -
bit 1: Display: -More- Available (1 on, 0 off)



bit 3: Display: Picture Caller-ID (1 on, 0 off)



bit 6: WebAccess > Stored Pages Menu (1 on, 0 off) (menu item, may require update to mma files)



bit 7: Browser: Browser Callback (1 on, 0 off)

offset 5B -
bit 0: WebAccess > Web Shortcuts (1 on, 0 off) (menu item, may require update to mma files)



bit 2: WebAccess > Browser History (1 on, 0 off) (menu item, may require update to mma files)



bit 3: Browser: Browser > Menu > Reload (Reload URL) (1 on, 0 off)



bit 6: Browser: Copy Text (1 on, 0 off)



bit 7: Browser: Copy All (1 on, 0 off)

offset 5C - 
bit 0: Browser: Browser > Menu > Exit (1 on, 0 off)



bit 1: Browser: Browser > Menu > View URL (1 on, 0 off)



bit 2: WebAccess > Go to URL Menu (1 on, 0 off) (menu item, may require update to mma files)



bit 4: Browser: Use Cookies (1 on, 0 off)



bit 6: Phone Wakeup for Alerts (1 on, 0 off)



bit 7: Message > Browser Msgs > Menu > Brwsr Msg Setup > Msg Notification > Medium Priority (1 on, 0 off) (Required for T-Mobile USA customers utilizing the E-Mail Alerts Function)

offset 5D -
bit 1: Settings > Personalize > Ring Styles > Silent Details (1 on, 0 off)

offset 5E -
bit 5: MMS: MMS Available (1 on, 0 off)



bit 6: MMS > New Multimedia Message > Receipt > Delivery Report (1 on, 0 off)



bit 7: MMS > New Multimedia Message > Receipt > Read Report (1 on, 0 off)

offset 5F -
bit 1: Message > Menu > Message Setup > MMS Message Setup > Server Info, Activate Menu Key for New, Edit, Delete (1 on, 0 off)



bit 2: Message > Inbox Setup > MMS > Server Info > Edit (1 on, 0 off)



bit 3: Display: Show Sender ID on Summary View (1 on, 0 off)



bit 4: Personalize Right Soft Key (1 on, 0 off)



bit 5: Personalize Left Soft Key (1 on, 0 off)



bit 6: Webaccess > Web Sessions > Menu > Set Default (1 on, 0 off)



bit 7: Multimedia (1 on, 0 off)

offset 60 -
bit 0: 'GPRS Active' text with GPRS PDP Context Icons (1 on, 0 off)



bit 1: Settings > Java Settings > DNS IP viewable (1 on, 0 off)



bit 2: Settings > Java Settings > DNS IP changable (1 on, 0 off)



bit 6: Video Camera Support (1 on, 0 off)



bit 7: Settings > Security > Lock Application > Multimedia (1 on, 0 off)

offset 61 -
bit 1: External Storage Devices Available: MMC or SD Card Slot (1 on, 0 off)



bit 3: Office Tools > Datebook > Weekview (1 on, 0 off)



bit 4: Office Tools > Datebook > Monthview (1 on, 0 off)

offset 62 -
bit 1: WAP Support (1 on, 0 off)



bit 3: Settings > Connection > Sync (1 on, 0 off) (menu item, may require update to mma files)



bit 4: SMS: SMS Over GPRS Protocol Enable (1 on, 0 off)



bit 5: Messages > Message Setup > Use GPRS (1 on, 0 off)



bit 7: Browser: Dial Prompt Available (1 on, 0 off)

offset 63 -
bit 0: WebAccess > Web Sessions (1 on, 0 off)



bit 2: Settings > Ring Styles > Ring Lights (1 on, 0 off)



bit 4: Settings > Security > Lock Application > IM (1 on, 0 off)

offset 64-
bit 2: SIMTK In-Call Menu (1 on, 0 off)



bit 3: E-Mail WAP Push (1 on, 0 off)



bit 4: E-Mail SSL Support (1 on, 0 off)



bit 5: RE: In Subject (1 on, 0 off)



bit 6: FWD: In Subject (1 on, 0 off)

offset 65 -
bit 0: Settings > Ring Styles > Event Lights (funlight.pat required in /a/mobile/audio/) (1 on, 0 off)



bit 1: Office Tools > IM (1 on, 0 off) (menu item, may require update to mma files)



bit 2: Replace HOLD with MUTE Softkey (1 on, 0 off)



bit 3: MMS Invisible Downloads (Background) (1 on, 0 off)



bit 4: WebAccess/Internet (1 on, 0 off)



bit 6: Phonebook: Picture-ID Listings (1 on, 0 off)



bit 7: DRM FWD Lock and Combined Delivery (1 on, 0 off)

offset 66 -
bit 0: DRM Seperate Delilvery (1 on, 0 off)



bit 1: HTTP Capable (1 on, 0 off)



bit 2: SIMTK Set Playtone Volume (1 on, 0 off)



bit 3: Resize Images (1 on, 0 off)



bit 5: MMS Kb Counter (1 on, 0 off)



bit 6: SMIL Message Composer (1 on, 0 off)



bit 7: Soundtracks (1 on, 0 off)

offset 67 -
bit 4: Display call divert/forward icon on line 1 and status on line 3 (1 on, 0 off) (must be on if offset 02, bit 4 is on)



bit 6: Display Thumbnails in Multimedia > Pictures (1 on, 0 off)



bit 7: Send To New Phonebook Entry (1 on, 0 off)

offset 68 -
bit 0: Settings > Initial Setup > Vibe Sync (1 on, 0 off)



bit 2: MMS Postcard (1 on, 0 off)



bit 3: MMS Templates Available (1 on, 0 off) (see also offset 6B, bit 7)



bit 4: GPRS Packet Data Transfer Icon (1 on, 0 off)



bit 6: Message > Create Message > New Letter (1 on, 0 off)

offset 69 -
bit 3: Multi-page SMS Send Confirmation (greater than 160 characters) (1 on, 0 off)



bit 4: File Manager (1 on, 0 off)



bit 5: Insert Phonebook Number In Msg Body (1 on, 0 off

offset 6A -
bit 0: Audio Player (1 on, 0 off)



bit 1: Multimedia > Pictures > Picture Viewer > Resolution (1 on, 0 off)



bit 3: Settings > Initial Setup > Display Timeout (1 on, 0 off)



bit 4: Multimedia > Pictures > Picture Viewer > Slideshow (1 on, 0 off)



bit 5: Multimedia > Sounds > Audio Player > Playlist (1 on, 0 off)



bit 6: Multimedia > Auto Timer (Sounds and Pictures) (1 on, 0 off)



bit 7: PC to Phone Transfer (1 on, 0 off)

offset 6B -
bit 0: BlueTooth OBEX (1 on, 0 off)



bit 1: Browser: Delete Cache On Exit (1 on, 0 off)



bit 4: default curser position on main menu when viewed by icon (1 center, 0 top left)



bit 5: GPRS Packet Data Icon (1 on, 0 off)



bit 6: VM message counter in Messages > Voicemail (0 on, 1 off)



bit 7: Message > MMS Templates (1 on, 0 off) (see also offset 68, bit 3)

offset 6C -
bit 0: Keypad: 5-Way Nav Key (1 on, 0 off)



bit 1: WebAccess > Browser (show address bar) (1 on, 0 off)



bit 3: BLOCK/LIMIT: Settings > Personalize > Home Screen > Home Keys (limited), Layout (blocked) (1 on, 0 off - set to 0 to UNBLOCK/UNLIMIT these features)



bit 5: Multimedia > Camera > Brightness (1 on, 0 off)

offset 6D -
bit 5: Silent Alerts Set At 0 (1 on, 0 off)



bit 7: Cingular Custom Prompts (1 on, 0 off)

offset 6E - 
bit 1: remove right soft key on home screen for custom branding (ie. Vodaphone Live!) (1 on, 0 off)



bit 2: Multimedia > Video > Menu > Videos Setup > Recording Sound (1 on, 0 off)



bit 3: Multimedia > Video > Menu > Videos Setup > Length (1 on, 0 off)



bit 4: Multimedia > Video (1 on, 0 off) (menu item, may require update to mma files)

offset 6F -
bit 0: Multimedia > Camera > Zoom (1 on, 0 off)



bit 2: Multimedia > Videos/Pictures/Sounds > Auto Repeat (1 on, 0 off)



bit 3: Multimedia > Videos/Pictures/Sounds > Shuffle (1 on, 0 off)



bit 4: Multimedia > Sounds/Videos > Menu > Sounds/Videos Setup > Timer (1 on, 0 off)



bit 5: Multimedia > Pictures > Menu > Pictures Setup > Counter (1 on, 0 off)



bit 6: Multimedia Allow Alerts (1 on, 0 off)



bit 7: Multimedia > Video > Menu > Videos Setup > Video Quality (1 on, 0 off)

offset 70 -
bit 0: Multimedia > Video > Menu > Videos Setup > Lighting Condition (1 on, 0 off)



bit 1: Multimedia > Camera/Video > Setup > Exposure (1 on, 0 off)



bit 2: Multimedia > Camera > Setup > Shutter Tone (1 on, 0 off)



bit 3: Multimedia > Camera > Setup > Mirror (1 on, 0 off) (can cause 'picture failed' errors)



bit 4: Multimedia > Camera > Menu > Pictures Setup > Status Icons (1 on, 0 off)



bit 5: Allow Shutter Tone NONE Option (1 on, 0 off)



bit 6: Multimedia > Video Camera (1 on, 0 off)  (see also seem 004a, offset 1D3) (menu item, may require update to mma files)

offset 71 -
bit 0: Vibrate Fix for V180 Phones Flashed with V220 Firmware



bit 1: Browser (Only if No WebAccess Supported Menu) (1 on, 0 off)



bit 4: Settings > Java Settings > Switching to Debug option (1 on, 0 off)



bit 6: Games & Apps display splash screen (1 on, 0 off)



bit 7: Settings > Java Settings > Start TCK (1 on, 0 off)

offset 72 - 
bit 0: J2ME: Tell A Friend Option (Games and Apps) (1 on, 0 off)



bit 1: Settings > Java Settings > App Priority, Set Standby App, App Backlight/Blink (1 on, 0 off)



bit 5: Browser: Cache (1 on, 0 off)



bit 6: Multimedia: Image Style Support (1 on, 0 off)



bit 7: Dynamic Prompts (/a/dnp.prf) changes message names (0 for 'Short Msg, MMS' , 1 for 'Text Msg, Multimedia') **FLEX Dependent

offset 73 -
bit 1: Camera > Store Options > Send to My Album (1 on, 0 off) (**OPERATOR / FLEX Dependent**)



bit 7: Settings > Security > Lock Application > BlueTooth (1 on, 0 off)

offset 74 - 
bit 4: provider tag (1 to remove, 0 to display) (offset 4B, bit 6 must be set to 0) (removes justification on home screen, Settings > Personalize > Home Screen > Layout, causes lines of 000-000 to display at Settings > Network > Available Networks)



bit 6: Settings > Initial Setup > Brightness (1 on, 0 off)

offset 75 -
bit 4: Settings > Call Forwarding 'detailed' option added (1 on, 0 off)



bit 5: Settings > Initial Setup > Display Timeout > 5 and 10 minutes (0 on, 1 off)



bit 7: Display MMS Progressbar (1 on, 0 off)

offset 76 -
bit 2: Allow MSG Edit On Resend (1 on, 0 off)



bit 3: Hide Edit On Resend Confirmation Dialogue (1 on, 0 off)



bit 4: Remove TO: Field From Reply (1 on, 0 off)



bit 5: Show Web Browser Loading Status Animations (1 on, 0 off)



bit 7: Browser: Title Scroll Support (1 on, 0 off)

offset 77 -
bit 0: Browser: URL as Title (1 on, 0 off)



bit 6: Multimedia > Camera (1 on, 0 off)

offset 78 -
bit 0: Display MMS Status Pop-Up (1 on, 0 off)



bit 3: Multimedia > Pictures > Menu > Send as TIM Click (1 on, 0 off) (language pack dependent)

offset 79 -
bit 1: Keypad: Camera Key (1 on, 0 off)



bit 4: Flashlight in Multmedia > Camera > Pictures (E398) (1 on, 0 off)



bit 5: Use Info Services Alert for Browser Msg (1 on, 0 off)



bit 6: SMS Subject (1 on, 0 off)

offset 7A -
bit 4: Vibe and Ring (E398/V551) (1 on, 0 off)



bit 7: Settings > Phone Status > Other Information > Operator (1 on, 0 off)

offset 7B -
bit 2: Personalize > Phone Status > Software Update (1 on, 0 off)

offset 7C -
bit 1: Display: WVIM Branding Support (1 on, 0 off)



bit 2: Show signal, time, battery status when display goes to blank (1 on, 0 off) (Settings > Initial Setup > Display Timeout must be 1 or 2 minutes)

offset 7D -
bit 5: Alert Ramp Up (Increasingly Louder Ringtone) (1 on, 0 off)



bit 7: Multimedia > Video > Menu > Videos Setup > Resolution (1 on, 0 off)

offset 7E -
bit 0: Handsfree immediately available when starting a call (1 on, 0 off)



bit 1: Multimedia > Videos > Videos Setup > Zoom (1 on, 0 off)

offset 7F -
bit 0: Message > Message Setup > MMS Message Setup, Size Limit (1 on, 0 off)



bit 1: Auto Network on Power Up (1 on, 0 off)

offset 80 - 
bit 2: Poll Headset for TTY Call (1 on, 0 off)



bit 6: Settings > Initial Setup > Backlight length options (1 for 20/40/60 seconds, 0 for 5/10/20 seconds)

offset 81 -
bit 2: Multimedia > Videos > Videos Setup > Styles > Black and White (1 on, 0 off) (offset 82, bit 0 must be set to 1)



bit 3: Multimedia > Videos > Videos Setup > Styles > Bluish (1 on, 0 off) (offset 82, bit 0 must be set to 1)



bit 4: Multimedia > Videos > Videos Setup > Styles > Antique (1 on, 0 off) (offset 82, bit 0 must be set to 1)



bit 5: Multimedia > Videos > Videos Setup > Styles > Reddish (1 on, 0 off) (offset 82, bit 0 must be set to 1)



bit 6: Multimedia > Videos > Videos Setup > Styles > Greenish (1 on, 0 off) (offset 82, bit 0 must be set to 1)



bit 7: Multimedia > Videos > Videos Setup > Styles > Negative (1 on, 0 off) (offset 82, bit 0 must be set to 1)

offset 82 -
bit 0: Multimedia > Videos > Videos Setup > Styles (1 on, 0 off)



bit 1: Multimedia > Video Camera > Brightness Adjustment (1 on, 0 off)



bit 2: Display: Allow Screensaver If J2ME Active (1 on, 0 off)



bit 6: Keynote Sound for Keypresses (1 on, 0 off)



bit 7: Multimedia > Videos > Videos Setup > Video Length (1 on, 0 off)

offset 83 -
bit 4: right softkey function after taking picture/video (1 SEND, 0 STORE)



bit 7: USB Settings (1 on, 0 off)

offset 84 -
bit 3: Multimedia > Pictures > Pictures Setup > Image Style (1 on, 0 off)



bit 4: Create Message > MMS > Priority > Low (1 on, 0 off)



bit 5: SIMTK Refresh: No Please Wait Notice (1 on, 0 off)

offset 85 -
bit 2: Multimedia > Camera > Camera Setup > Resolution (1 on, 0 off)



bit 4: Multimedia > Camera > Camera Setup > Auto Timer (1 on, 0 off)



bit 6: Airplane Mode Lock (1 on, 0 off) (menu item, may require update to mma files) (confirmed not to work on V551)



bit 7: Enhanced Fixed Dial (1 on, 0 off)



bit 7: CPHS Orange Available (1 on, 0 off)

offset 86 -
bit 1: Call Barring > BOAC Available (1 on, 0 off)



bit 2: Call Barring > BOIC Available (1 on, 0 off)



bit 3: Call Barring > BOIC_EXHC Available (1 on, 0 off)



bit 4: Call Barring > BAIC Available (1 on, 0 off)



bit 5: Call Barring > BIC Roam Available (1 on, 0 off)



bit 6: Call Barring > CLIP Available (1 on, 0 off)



bit 7: Line 2 Call Forward

offset 87 -
bit 0: Line 2 Conditional Call Forward (1 on, 0 off)



bit 1: Line 2 If Busy, then Call Forward (1 on, 0 off)



bit 2: Line 2 If No Answer, then Call Forward (1 on, 0 off)



bit 3: Line 2 If Not Reachable, then Call Forward (1 on, 0 off)



bit 4: Line 2 Call Barring (1 on, 0 off)



bit 5: Call Barring > BOAC Line 2 Available (1 on, 0 off)



bit 6: Call Barring > BOIC Line 2 Available (1 on, 0 off)



bit 7: Call Barring > BOIC_EXHC Line 2 Available (1 on, 0 off)

offset 88 -
bit 0: Call Barring > BAIC Line 2 Available (1 on, 0 off)



bit 1: Call Barring > BIC Roam Line 2 Available (1 on, 0 off)



bit 2: Line 2 Call Hold (1 on, 0 off)



bit 3: Line 2 Call Waiting (1 on, 0 off)



bit 4: MT SMS Line 2 (1 on, 0 off)



bit 5: MO SMS Line 2 (1 on, 0 off)



bit 6: CLIP Line 2 Available (1 on, 0 off)



bit 7: Allow CLI Send (Calling Line Identifier) Line 2 (1 on, 0 off)

offset 89 -
bit 0: Allow CLI Block (Calling Line Identifier) Line 2 (1 on, 0 off)



bit 1: Voicemail Line 2 Available (1 on, 0 off)



bit 2: EDGE Icon (1 on, 0 off) (only on EDGE supported phones with late version firmware)



bit 5: Swap Softkeys (1 on, 0 off)



bit 6: Multimedia > Camera > Camera Setup > Image Quality (1 on, 0 off)

offset 8A -
bit 1: Multimedia > Videos > New Video > Pause/Resume Capture (1 on, 0 off)



bit 2: Speaker Call to End on Flip Close (1 on, 0 off)

offset 8B -
bit 1: Allow DRM File Download To Ext Storage (1 on, 0 off)



bit 2: Multimedia Video Player Stretch Video (1 on, 0 off)



bit 4: Cingular ENS Capable (1 on, 0 off)



bit 7: Multiple Skin Support (1 on, 0 off)

offset 8C -
bit 0: Multimedia: Store> Store Options > Send Postcard



bit 2: Allow Use of Pictures on Removable Media for Phonebook (1 on, 0 off)

offset 8D -
bit 0: USSD Alert Available (1 on, 0 off)



bit 4: UMAN Feature Enabled (1 on, 0 off)

offset 93 -
bit 0: V3i: Settings > Phone Status (1 on, 0 off)



bit 1: V3i: Settings > Personalize (1 on, 0 off)



bit 2: V3i: Settings > Network (1 on, 0 off)



bit 3: V3i: Settings > Ring Styles (1 on, 0 off)



bit 4: V3i: Settings > Security (1 on, 0 off)



bit 5: V3i: Settings > Initial Setup (1 on, 0 off)



bit 7: V3i: Messages, blue Message button (1 on, 0 off)

offset 94 -
bit 0: V3i: Settings > Car Settings (1 on, 0 off)



bit 1: V3i: Settings > Headset (1 on, 0 off)



bit 3: V3i: Settings > In-Call Setup (1 on, 0 off)



bit 4: V3i: Phonebook (1 on, 0 off)



bit 5: V3i: Tools > Shortcuts (1 on, 0 off)

offset 96 -
bit 4: V3i: Camera Orientation (1 normal, 0 flipped horizontal and vertical)

offset 9A - 
bit 7: Multimedia > Sounds > Playlist capability, ability to 'hide' sound player (0 on, 1 off)

offset AE -
bit 0: V3i: Camera IU (1 transparent, 0 opaque/V3 style)

========

spcolor.sch

upload to /a/mobile/system/

activate bit #6 of offset 53 in seem 0032_0001

**thanks to poesjeNL and FlyingHorse for the English translation**

034 - background color messages

038 - background color main menu

03C - color of characters in menu and the inner color of the characters on the main screen

040 - color of the text of a selected item

044 - color of the text at the discription of the pictures/ringtones/video

048 - ???

04C - textcolor of calendar entry for "today"

050 - ???

054 - color of hour- and minute-hands on analog clock

058 - border color the text on the main screen

05C - textcolor of the bottom bar

060 - textcolor at button press

064 - textcolor titlebar (main menu)

068 - textcolor titlebar (submenu/input area)

06C - upper color selection bar

070 - bottom color selection bar

074 - color line above bottom bar and right of scroll-bar

078 - upper color bottom bar

07C - bottom color bottom bar

080 - upper color of pressed button

084 - bottom color of pressed button

088 - upper color titlebar (above main menu)

08C - bottom color titlebar (above main menu)

090 - upper color titlebar (above submenu and input)

094 - bottom color titlebar (above submenu and input)

098 - color right line of horizontal bar at files (pictures/ringtones/filmpjes)

09C - background color of iTap line, symbols that are not active

0A0 - background color of calculator

0A4 - background color input/selection area

0A8 - background color of the information at multimedia (pictures/ringtones/video)

0AC - color of line under the input area

0B0 - color of line under the input area when selected

0B4 - color of cursor at input

0B8 - ???

0BC - horizontal line in calendar

0C0 - vertical line in calendar

0C4 - main color in calendar (weeks/months)

0C8 - background color of calendar entry for "today"

0CC - horizontal solution line in calculator (between 2+2 and 4)

0D0 - "emergency call" upper color titlebar

0D4 - "emergency call" bottom color titlebar

0D8 - "emergency call" color of line surrounding input area and titlebar

0DC - color of line surrounding icons

0E0 - color of line surrounding upper side of input area

0E4 - color of line surrounding bottom side of input area

0E8 - color of line surrounding submenu's and left and right sude of input area

0EC - color 1e line of scroll-bar

0F0 - color 2e line of scroll-bar

0F4 - background color of scroll-bar

0F8 - color bottom of scroll-bar

0FC - color of upper/left side of scroll block when playing a video

100 - upper background color of the bar at multimedia (under pictures/ringtones/videos/camera)

104 - bottom background color of the bar at multimedia (under pictures/ringtones/videos/camera)

108 - upper color of scroll-bar

10C - ???

110 - ???

114 - ???

118 - background color of a selected main menu item

11C - background color of the text at the buttond/options under the camera

120 - color for links in sound/pictures menu (certain branded flexes only)

124 - ???

128 - color for links in sound/pictures menu when highlighted (certain branded flexes only)

12C - ???

Specify colors in spcolor.sch in hexadecimal RGB.

The offset specified is the starting point - each six digit color is actually stored in three successive offsets.

For example: offset 78, upper color bottom bar: if you want the color FF1432, put "FF" in offset 78, "14" in offset 79, and "32" in offset 7A.

Certain fields can have transparency - that is the fourth successive offset, specify transparency amount from 00 to FF.  This will not work for all color settings.

